{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["VM Load Results 3 Caps"],"read":"whole","date_system":"1900"}

{"sheet":"VM Load Results 3 Caps","index":0,"n_rows":34,"n_cols":21,"rows_kept":34,"merged":[[1,0,1,1],[2,4,2,5],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,5],[7,6,8,6],[7,7,8,7],[7,8,8,8],[7,9,8,9],[7,10,7,11],[7,12,7,13],[7,14,8,14],[7,15,7,16],[7,17,7,20],[16,0,16,1],[17,0,17,5],[18,0,18,5],[19,0,19,5],[20,0,20,5],[21,0,21,5],[22,0,22,5],[23,0,23,5],[24,0,24,5],[26,0,26,1],[27,0,27,5],[28,0,28,5],[29,0,29,5],[30,0,30,5],[31,0,31,5],[32,0,32,5],[33,0,33,5]]}
[]
["FS host specs"]
["CPU","2 core"]
["RAM","8GB"]
["HDD","80GB"]
[]
[]
["CAPS","VM Duration","Load Duration(in mins)","Total call attempts ","Successful calls","Successful deposits","Simultaneous deposits","Avg CPU usage (%)","Memory usage(Gb)","FS instance","Before Load",null,"After Load",null,"Peak \nCPU Usage(%)","Network Interface",null,"IOPS"]
[{"$nulls":10},"Commitlog","Data","Commitlog","Data",null,"Bytes Received/Sec","Bytes Sent/Sec","Read Bytes/Sec","Write Bytes/Sec","Reads/Sec","Writes/Sec"]
[3,30,720,136655,136655,136655,120,65,3.9,"FS1","64mb","2.89mb","1gb","1.34gb",88,878969,4117268,74.43,2633333,0.005,25.4]
[{"$nulls":7},20,1.7,"FS2","64mb","2.76mb","1gb","1.28gb",60,1377006,17343,746.6,2472065,0.003,24.14]
[{"$nulls":7},19,1.7,"FS3","64mb","2.76mb","1gb","1.29gb",61,1390856,14356,11045,2470293,0.104,25.6]
[{"$nulls":7},21,1.7,"FS4","64mb","2.73mb","1gb","1.11gb",61,1256979,27293,1894,2343501,0.078,24.5]
[]
[]
[]
["Environment Configurations"]
["Single site and 4 Feature Servers without N+1 HA"]
["All the 4 Feature Servers are connected to 1 SIP Switch"]
["SIPS Dial-Plan "]
["Windows 2008 OS"]
["Feature Server virtual machine has 2 core CPU, 8 GB RAM and 80 GB hard disk. "]
["200 DNs and each DN associated with a mailbox"]
["Voicemails are deposited on DNs mailboxes and all the DNs are statically associated with Persons"]
["FS Version 8.1.201.42 "]
[]
["Voicemail Configurations"]
["IVR profile is used to send http requests from MCP to FS1. "]
["voicemail-quorum = True"]
["replication_factor = 3"]
["Log Level = Standard "]
["voice-mailbox-message-count = 1000"]
["voice-message-max-duration = 60"]
["All modules such as DM and FS Dial-plan are disabled."]